For 1990-2009 cars

#### Tools Required

48000 Marson Plastic Rivet Setter

### Removal Procedure

1. Remove the cargo cover by disengaging the attaching rings from the plastic rivet fasteners in the rear of vehicle.
2. For removal of the plastic rivet fasteners drill out the center pin with a 5/32 in. drill bit.

### Installation Procedure

1. Install the plastic rivets into the trim panel using a Marson Plastic Rivet Setter 48000 (or equivalent).
2. Position the cargo cover with the attaching rings in the forward position of the vehicle. Slip the attaching rings over the retainers in the rear end panel at the wheelhouse area.
3. Secure the rear of the cargo cover to the vehicle at the convenience net upper attachment locations.