For 1990-2009 cars

### Removal Procedure

1. Remove the carpet. Refer to Floor Panel Carpet Replacement .
2. Remove the carpet block by disengaging the clock key from under the left parking brake cable.

### Installation Procedurea

1. Slide the carpet block key under the left parking brake cable and up against the parking brake cable retention bracket.
2. Install the carpet into the vehicle. Refer to Floor Panel Carpet Replacement .