For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Drums

- Runout

0.15 mm

0.006 in

- Inside Diameter

200.0 mm

7.87 in

- Maximum Refinish Diameter

200.6 mm

7.90 in

- Discard Diameter*

201.4 mm

7.93 in

Brake Rotors

- Lateral Runout

0.060 mm

0.0024 in

- Thickness Variation

0.013 mm

0.0005 in

- Diameter

250.5 mm

9.86 in

- New Thickness (Nominal)

18.0 mm

0.710 in

- Minimum Thickness After Refinish

16.1 mm

0.633 in

- Discard Thickness*

15.8 mm

0.625 in

Brake Linings

- Front Disc Pads

- New Thickness

11.0 mm

0.43 in

- Discard Thickness

2.0 mm

0.08 in

- Rear Drum Shoes

- New Thickness

4.0 mm

0.16 in

- Discard Thickness

1.0 mm

0.04 in

Hub and Bearing Assemblies

- Front

- End Play

0.020 mm

0.001 in

- Lateral Runout

0.040 mm

0.0016 in

- Rear

- End Play

0.130 mm

0.005 in

- Lateral Runout

0.050 mm

0.002 in

- Radial Runout

0.130 mm

0.005 in

Master Cylinder Bore Diameter | 22.2 mm | 0.87 in
Caliper Bore Diameter | 51.0 mm | 2.01 in
Wheel Cylinder Bore Diameter | 19.0 mm | 0.75 in
Minimum Vacuum at Power Booster | -- | 15 in Hg
Brake System Fluid Capacity | 0.5 liters | 17.0 oz
*Brake drums and rotors have a discard diameter or thickness dimension cast into them. This is a wear dimension and not a refinish dimension. Any drum or rotor which does not meet the specification values should be discarded.