For 1990-2009 cars

### Disassembly Procedure

1. While holding the fan, remove the fan to motor nut (left hand thread) and pull the fan off of the motor shaft.
2. Remove the screws holding the fan motor to the shroud.
3. Remove the motor from the fan shroud.

### Assembly Procedure

1. Install the motor in the shroud.

Notice: Refer to Fastener Notice in the Preface section.

2. Install and tighten the fan motor-to-shroud screws.

Tighten
Tighten the fan motor-to-shroud screws to 4 N·m (35 lb in).

3. Install the fan on the motor shaft.
4. Install and torque the fan nut.

Tighten
Tighten the fan nut to 3-5 N·m (27-44 lb in).