For 1990-2009 cars

### Removal Procedure

1. Remove inner panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove rear door inner belt seal. Refer to Rear Door Window Belt Inner Sealing Strip Replacement .
3. Lower door window to full down position.
4. Remove seal from door header flange and rear door stationary window.

### Installation Procedure

1. Install seal to rear door header flange and rear door fixed window guide.
2. Install rear door inner belt seal. Refer to Rear Door Window Belt Inner Sealing Strip Replacement .
3. Install rear door inner panel. Refer to Rear Side Door Trim Panel Replacement .