For 1990-2009 cars

## Energy Absorber Pad Replacement - Center Pillar Lower Sedan/Wagon

### Removal Procedure

Caution: If energy absorber is removed or damaged it must be replaced with a new part. If omitted, the vehicle will not meet federal motor vehicle safety standards (FMVSS), subjecting the retailer to possible civil penalties for making the vehicle inoperative to the FMVSS, and increasing the risk of injury to the vehicle occupants.

1. Remove the center pillar lower trim finish panel. Refer to Center Pillar Garnish Molding Replacement .
2. Remove the energy absorber by pulling.

### Installation Procedure

1. Install the center pillar lower energy absorber.
2. Install the center pillar lower trim finish panel. Refer to Center Pillar Garnish Molding Replacement .