For 1990-2009 cars

### Circuit Description

3rd clutch is applied when circuit 1223 is opened at the powertrain control module (PCM). When the PCM opens the circuit the voltage is monitored at terminal J4A06 to check for propper circuit conditions.

### DTC Parameters

DTC P0761

### Conditions for Setting the DTC

### Action Taken When the DTC Sets

### Conditions for Clearing the MIL/DTC

### Diagnostic Aids