For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the plastic retainers from the cradle and the air duct inlet.

### Disassembly Procedure

1. Unhook the springs at the rear of the air deflector.
2. Remove the deflector from the splash shield.

### Assembly Procedure

1. Insert the springs through the holes in the air deflector and the splash shield.
2. Hook the springs at each end of the deflector together.
3. Check the forward and rearward movement of the air deflector.

### Installation Procedure

1. Position the air deflector to the vehicle and install the plastic retainers.
2. Lower the vehicle.