For 1990-2009 cars

#### Tools Required

SA9103E Regulator Valve Remover/Replacer

1. Install the relief valve and oil pump assembly.
2. If the relief valve was removed, replace it with a new one. Coat the valve with engine oil and tap it into the cover bore until it seats using the SA9103E and a hammer.

Important: If removed, the oil pump assembly must be packed with petroleum jelly to prime the pump.

3. Install the drive and driven rotors into the pump body with the chamfer toward the front oil seal.

Notice: Make sure the nine holes in the front cover are clean. The oil pump cover screws are coated with a sealant to prevent oil leakage. New screws must be installed.

4. Install the pump body cover with new screws.

Tighten
Tighten the screws to 11 N·m (97 lb in).