For 1990-2009 cars

Table 1: | Air Pump
Table 2: | Air Pump Solenoid-1999 Only
Table 3: | Crankshaft Position Sensor
Table 4: | Electronic Ignition Module
Table 5: | Engine Coolant Temperature Sensor
Table 6: | Evaporative Cannister Vent Valve
Table 7: | Evaporative Emission Cannister Purge Solenoid
Table 8: | EVO Solenoid
Table 9: | Fuel Injectors-1&2
Table 10: | Fuel Injector-3&4
Table 11: | Fuel Tank Pressure Sensor
Table 12: | Fuel Tank Unit
Table 13: | Generator-1998 1st Design Only
Table 14: | Generator
Table 15: | Heated Oxygen Sensor
Table 16: | Idle Air Control
Table 17: | Ignition Switch
Table 18: | Intake Air Temperature Sensor
Table 19: | Knock Sensor
Table 20: | Linear EGR Solenoid
Table 21: | Manifold Absolute Pressure (MAP) Sensor-Manual
Table 22: | Manifold Absolute Pressure (MAP) Sensor-Auto
Table 23: | Oil Pressure Switch
Table 24: | Oxygen Sensor
Table 25: | Park/Neutral Position Switch
Table 26: | Park/Neutral Position Switch
Table 27: | Park/Neutral Position Switch
Table 28: | Powertrain Control Module (PCM) --J1-LT BLU
Table 29: | Powertrain Control Module (PCM)-J2-LT BLU
Table 30: | Powertrain Control Module (PCM)-Automatic J3 --PNK
Table 31: | Powertrain Control Module (PCM)-Manual J3-BRN
Table 32: | Powertrain Control Module (PCM)-Automatic J4
Table 33: | Starter Relay
Table 34: | Throttle Position Sensor (TPS)

#### Air Pump

Connector Part Information |

• | 12192968

• | Gray

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | RED | 78 | 2.0 | AIR PUMP RELAY
B | BLK | 651 | 2.0 | GROUND
Location: Engine Compartment -- Front Center

#### Air Pump Solenoid-1999 Only

Connector Part Information |

• | 12105333

• | Brown

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | PNK/BLK | 429A | .35 | PCM
B | BLK | 639X | .35 | IGNITION
Location: Engine Compartment -- Front Center

#### Crankshaft Position Sensor

Connector Part Information |

• | 12052642

• | Green

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | PPL | 574-AUTO 574M-Man | .35 | 7X REF-LO
B | YEL | 573-AUTO 573M-Man | .35 | 7X REF-HI
Location: Engine Compartment-On Lower Rear of Block

#### Electronic Ignition Module

Connector Part Information |

• | 12160397

• | Green

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | PNK | 1039 | .35 | IGN1
B | BLK/WHT | 451C | .35 | GROUND
C | ORN | 406 | .35 | EST2-3 IN
D | BRN/WHT | 633-AUTO 633M-Man | .35 | CYLINDER 4 SIGNAL OUT
E | WHT | 423 | .35 | EST 1-4 IN
Location: Engine Compartment-Center Front

#### Engine Coolant Temperature Sensor

Connector Part Information |

• | 12092512

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | YEL | 410 | .35 | SENSOR INPUT SIGNAL
B | BLK | 452MA-Man 452M-Auto | .35 | RETURN
Location:Engine Compartment-Upper Left

#### Evaporative Cannister Vent Valve

Connector Part Information |

• | 12052643

• | Red

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | PNK | 39T | .35 | IGN
B | WHT | 1310B | .35 | TO PCM
Location: On Fuel Filter Neck

#### Evaporative Emission Cannister Purge Solenoid

Connector Part Information |

• | 12052643

• | Red

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | PNK | 639B | .50 | IGN1
B | DK GRN/WHT | 428 | .50 | SOLENOID CONTROL
Location: Engine Compartment-Lower Rear on Block

#### EVO Solenoid

Connector Part Information |

• | 12052643

• | Red

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BRN | 1295B | .35 | EVO LOW
B | WHT | 1294B | .35 | EVO HI
Location: Engine Compartment-On Bottom of Power Steering Pump

#### Fuel Injectors-1&2

Connector Part Information |

• | 12084126

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
1 | PNK | 139A139B | .80 .80 | B+ INJ 1 B+ INJ2
2 | BLK LT GRN/BLK | 1744 1745 | .80 .80 | PCM CONT. INJ1 PCM CONT> INJ2

#### Fuel Injector-3&4

Connector Part Information |

• | 12084126

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
1 | PNK | 139C 139E | .80 .80 | B+ INJ3 B+ IJN4
2 | PNK/BLK LT BLU/BLK | 1746 844 | .80 .80 | PCM CONT. INJ3 PCM CONT. INJ4
Location: Engine Compartment-Rear

#### Fuel Tank Pressure Sensor

Connector Part Information |

• | 12059595

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | ORN/BLK | 469B | .35 | RETURN
B | DK GRN | 890B | .35 | TO PCM
C | GRA | 416J | .35 | 5 V REF
Location: Rear Compartment-Left

#### Fuel Tank Unit

Connector Part Information |

• | 12162189

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | GRA | 120A 120B | .80 | FUEL PUMP FEED
B | BLK/WHT | 251B 251C | .80 | FUEL LEVEL SENSOR
C | PPL | 30B | .80 | FUEL LEVEL SENSOR
D | BLK | 550Z 550EE | .80 | W/ ABS GROUND W/O ABS GROUND
Location: Top of Fuel Tank

#### Generator-1998 1st Design Only

Connector Part Information |

• | 12191366

• | Gray

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | -- | -- | -- | --
B | BRN/WHT | 25A | .35 | BATT CHARGE TT
C | BRN | 641 | .35 | IGN
D | -- | -- | -- | --
Location: Engine Compartment-Lower Rear

#### Generator

Connector Part Information |

• | 15305338

• | Brown

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | -- | -- | -- | --
B | BRN/WHT | 25A | .35 | BATT CHARGE TT
C | BRN | 641 | .35 | IGN
D | -- | -- | -- | --
Location: Engine Compartment-Lower Rear

#### Heated Oxygen Sensor

Connector Part Information |

• | 12160482

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK/WHT | 451L | .50 | O2 SIGNAL GROUND
B | PPL/WHT | 1668-AUTO 1668M-MAN | .35 | O2 RETURN
C | DK GRN | 1423 | .35 | O2 HEATER GROUND
D | PNK | 639E | .80 | O2 HEATER FEED
Location: Top of Rear Cradle Cross Member

#### Idle Air Control

Connector Part Information |

• | 12162190

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | LT GRN/BLK | 444A | .35 | IAC B LO
B | LT GRN/WHT | 1749 | .35 | IAC B HI
C | LT BLU/BLK | 1748 | .35 | IAC A LO
D | LT BLU/WHT | 1747 | .35 | IAC A HI
Location: Engine Compartment-Center Rear Upper

#### Ignition Switch

Connector Part Information |

• | 12064998

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | RED | 102A | 3.0 | B+
B | ORN | 300 | 3.0 | IGNITION SW OUTPUT- IGN 3
C | YEL | 5 | 2.0 | CRANK OUTPUT
D | LT GRN | 80 | .35 | KEY MINDER SW SIGNAL
E | BLK | 350V | .35 | GROUND
F | PNK | 3C | 2.0 | IGNITION SW OUTPUT-IGN 1
G | BRN | 4 | 2.0 | ACC OFF/RUN
H | RED | 202 | 3.0 | B+
Location: Steering Column

#### Intake Air Temperature Sensor

Connector Part Information |

• | 12092512

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | TAN | 472A | .35 | IAT SENSOR SIGNAL
B | BLK | 452N-AUTO 452M-MAN | .35 | IAT SENSOR RETURN
Location: Engine Compartment-Front Left

#### Knock Sensor

Connector Part Information |

• | 12176800

• | Gray

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | DK BLU | 496-AUTO 496M-MAN | .35 | KNOCK SENSOR SIGNAL
Location: Rear Engine Block above Starter

#### Linear EGR Solenoid

Connector Part Information |

• | 12186057

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | LT BLU | 697B-SOHC 697-DOHC | .50 | LINEAR EGR SOLENOID CONTROL
B | BLK | 452GG-SOHC 452G-DOHC | .50 | RETURN TO PCM
C | BRN | 1456A-SOHC 1456-DOHC | .50 | LINEAR EGR FEEDBACK SIGNAL
D | GRA | 416EE-SOHC 416E-DOHC | .50 | 5 V REF
E | PNK | 639CC-SOHC 639C-DOHC | .50 | IGN FEED
Location: Engine Compartment-Camcover-DOHC Intake-SOHC

#### Manifold Absolute Pressure (MAP) Sensor-Manual

Connector Part Information |

• | 12020403

• | Green

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK | 452HM | .50 | MAP RETURN
B | LT GRN | 432A | .50 | MAP SIGNAL
C | GRA | 416F | .50 | MAP BATT
Location: Engine Compartment-Right Rear

#### Manifold Absolute Pressure (MAP) Sensor-Auto

Connector Part Information |

• | 12020403

• | Green

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK | 452HM | .50 | MAP RETURN
B | LT GRN | 432A | .50 | MAP SIGNAL
C | GRA | 416F | .50 | MAP BATT
Location: Engine Compartment-Right Rear

#### Oil Pressure Switch

Connector Part Information |

• | 12052644

• | Gray

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | TAN | 31A | .35 | OIL PRESSURE SW
B | -- | -- | -- | --
Location: Rear Engine Compartment Oil Filter

#### Oxygen Sensor

Connector Part Information |

• | 12089916

• | GrayON HERE

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | PPL | 412 | .80 | SIGNAL
Location: Engine Compartment-Center Front

#### Park/Neutral Position Switch

Connector Part Information |

• | 12059642

• | LT Gray

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | PPL | 6A | 3.0 | B+
B | PPL | 6X | 3.0 | FEED TO STARTER SOLENOID
Location: Engine Compartment-Lower Left

#### Park/Neutral Position Switch

Connector Part Information |

• | 12162260

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK/WHT | 771 | .50 | SHIFT SEL 1
B | YEL | 772 | .50 | SHIFT SEL 2
C | GRA | 773 | .50 | SHIFT SEL 3
D | WHT | 776 | .50 | SHIFT SEL D
E | LT GRN | 24C | .50 | REVERSE SWITCH
F | PNK | 239A | .50 | REVERSE SWITCH
Location: Engine Compartment-On Automatic Transaxle

#### Park/Neutral Position Switch

Connector Part Information |

• | 12089640

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK/WHT | 451K | 2.0 | GROUND
Location:Engine Compartment-On Automatic Transaxle

#### Powertrain Control Module (PCM) --J1-LT BLU

Connector Part Information |

• | 12110207-J1

• | Lt BLU

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
C1 | DK GRN | 335 | .35 | COOLING FAN RELAY CONTROL
C2 | TAN/BLK | 456 | .35 | UPSHIFT TT-MANUAL
C3 | BRN/WHT | 419 | .35 | MILTT OUT
C4 | YEL | 172 | .35 | LOW FUEL TT CONTROL
C5 | LT BLU | 1888 | .35 | CRUISE CLUTCH OUT
C6 | PPL | 1885 | .35 | SERVICE TT OUT
C7 | DK GRN | 35 | .35 | COOLANT HOT TT OUT
C8 | PPL | 1807A | .35 | CLASS 2-DLC
C9 | -- | -- | -- | --
C10 | DK GRN/WHT | 465 | .35 | FUEL PUMP RELAY OUT
C11 | DK GRN | 603 | .50 | A/C REQUEST INPUT
C12 | PNK | 439 | .35 | IGN 1
C13 | -- | -- | -- | --
C14 | BRN | 86B | .35 | BRAKE SWITCH INPUT
C15 | GRA | 1884 | .35 | CRUISE RASC IN
C16 | PPL/WHT | 455 | .35 | FUEL GAGE SIGNAL
D1 | GRA | 729 | .35 | A/C CLUTCH RELAY CONTROL
D2 | WHT | 121 | .35 | TACH OUT
D3 | DK GRN | 135 | .35 | COOL TEMP GAGE OUT
D4 | WHT | 1294A | .35 | EVO HI
D5 | BRN | 1295A | .35 | EVO LO
D6 | DK GRN | 389 | .35 | SPEED SIGNAL OUT
D7 | PNK | 1886 | .35 | CRUISE MOVE OUT
D8 | PPL | 1807B | .35 | CLASS 2 --ABS
D9 | DK BLU | 1446 | .35 | FLASH POWER
D10 | -- | -- | -- | --
D11 | LT GRN | 1887 | .35 | CRUISE WOT/IDLE OUT
D12 | -- | -- | -- | --
D13 | ORN | 1140 | .80 | 12 V BATT
D14 | LT BLU | 1344A | .35 | RKE TRUNK RELAY ENABLE
D15 | GRA | 416H | .35 | 5 V REF
D16 | BLK | 452K | .35 | FLASH RTN
Location: Behind Left Side of I/P

#### Powertrain Control Module (PCM)-J2-LT BLU

Connector Part Information |

• | 12110206-J2

• | LT BLU

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A1 | PNK/BLK | 1746 | .80 | CYL 3 INJ
A2 | LT BLU/BLK | 844 | .80 | CYL 4 INJ
A3 | LT GRN/BLK | 1745 | .80 | CYL 2 INJ
A4 | WHT | 1310A | .35 | EVAP VENT VALVE
A5 | BRN | 1456A 1456 | .50 | LIN EGR FEEDBACK IN-SOHC LIN EGR FEEDBACK IN-DOHC
A6 | DK BLU | 417A | .35 | TPS IN
A7 | LT GRN 432A |  | .50 | MAP IN
A8 | AN | 472A | .35 | INTAKE AIR TEMP SENSOR IN
A9 | LT GRN/WHT | 1749 | .35 | IAC B HI OUT
A10 | LT GRN/BLK | 444A | .35 | IAC B LO OUT
A11 | LT BLU/BLK | 1748 | .35 | IAC A LO OUT
A12 | LT BLU/WHT | 1747 | .35 | IAC A HI OUT
B1 | DK GRN/WHT | 428 | .50 | CCP OUT
B2 | BLK | 1744 | .80 | CYL 1 INJ
B3 | YEL | 410 | .35 | COOLANT TEMP IN
B4 | GRA | 416B | .35 | +5 V MAP/LEGR
B5 | GRA | 474 | .35 | +5 V TPS
B6 | BLK/WHT | 451E | .35 | GROUND
B7 | WHT | 423 | .35 | EST 1-4
B8 | ORN | 406 | .35 | EST 2-3
B9 | TAN/WHT | 551C 551A | .80 | GROUND-AUTO GROUND-MANUAL
B10 | LT BLU | 697B 697 | .50 | LIN EGR SOL OUT-SOHC LIN EGR SL OUT-DOHC
B11 | PNK | 639A | .50 | LIN EGR RECIRC
B12 | ORN | 1140A | .80 | 12 V BAT
Location: Behind Left Side of I/P

#### Powertrain Control Module (PCM)-Automatic J3 --PNK

Connector Part Information |

• | 12110245-J3

• | PNK

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
C1 | BLK/WHT | 1423A | .35 | HEATED O2
C2 | PNK/BLK | 429A | .35 | AIR PUMP SOLENOID-1999 ONLY
C3 | -- | -- | -- | --
C4 | YEL/BLK | 68A | .35 | COOLANT LEVEL IN
C5 | PPL | 30E | .35 | FUEL LEVEL IN
C6 | -- | -- | -- | --
C7 | BRN | 436 | .35 | AIR PUMP-1999 ONLY
C8-C9 | -- | -- | -- | --
C10 | DK BLU | 496 | .35 | KNOCK SENSOR IN
C11 | TAN | 413B | .80 | HO2S LO IN
C12 | PPL/WHT | 1668 | .35 | HO2S HI IN
C13 | TAN | 413A | .80 | O2 F LO IN
C14 | PPL | 412 | .80 | O2 F HI IN
C15 | PPL | 401 | .35 | VSS LO IN
C16 | BLK | 452G 452GG | .50 | LEGR RTN-DOHC LEGR RTN-SOHC
D1 | BLK | 452H | .50 | MAP RETURN
D2 | BLK/WHT | 251E | .35 | FUEL LEVEL RETURN
D3 | BRN/WHT | 633 | .35 | CYL #4 SIGNAL
D4-D6 | -- | -- | -- | --
D7 | DK GRN | 890A | .35 | FUEL TANK PRESSURE
D8 | BLK | 452MD | .35 | ECT SENSOR RETURN
D9 | ORN/BLK | 469B | .35 | FUEL TANK PRESSURE SENSOR RETURN-1999 ONLY
D10 | BLK | 452N | .35 | IAT SENSOR RETURN
D11 | BLK | 452J | .35 | TPS RETURN
D12 | -- | -- | -- | --
D13 | YEL | 573 | .35 | 7X HI IN
D14 | PPL | 574 | .35 | 7X LO IN
D15 | YEL | 400 | .35 | VSS HI IN
D16 | -- | -- | -- | --
Location: Behind Left Side of I/P

#### Powertrain Control Module (PCM)-Manual J3-BRN

Connector Part Information |

• | 12160779-J3

• | BRN

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
C1 | BLK/PWHT | 1423 | .35 | HEATED 02
C2 | PNK/BLK | 429A | .35 | AIR PUMP SOLENOID-1999 ONLY
C3 | -- | -- | -- | --
C4 | YEL/BLK | 68AM | .35 | COOLANT LEVEL IN
C5 | PPL | 30EM | .35 | FUEL LEVEL IN
C6 | -- | -- | -- | --
C7 | BRN | 436 | .35 | AIR PUMP-1999 ONLY
C8-C9 | -- | -- | -- | --
C10 | DK BLU | 496M | .35 | KNOCK SENSOR IN
C11 | TAN | 413BM | .80 | HO2S LO IN
C12 | PPL/WHT | 1668M | .35 | HO2S HI IN
C13 | TAN | 413AM | .80 | O2S F LO IN
C14 | PPL | 412M | .35 | O2S F HI IN
C15 | PPL | 401M | .35 | VSS LO IN
C16 | BLK | 452G 452GG | .50 | LEGR RTN-DOHC LEGR RTN-SOHC
D1 | BLK | 452HM | .50 | MAP RETURN
D2 | BLK/WHT | 251EM | .35 | FUEL LEVEL RETURN
D3 | BRN/WHT | 633M | .35 | CYL #4 SIGNAL
D4-D6 | -- | -- | -- | --
D7 | DK GRN | 890A | .35 | FUEL TANK PRESSURE
D8 | BLK | 452MB | .35 | ECT SENSOR RETURN
D9 | ORN/BLK | 469B | .35 | FUEL TANK PRESSURE SENSOR RETURN-1999 ONLY
D10 | BLK | 452NM | .35 | IAT SENSOR RETURN
D11 | BLK | 452JM | .35 | TPS RETURN
D12 | -- | -- | -- | --
D13 | YEL | 573M | .35 | 7X HI IN
D14 | PPL | 574M | .35 | 7X LO IN
D15 | YEL | 400M | .35 | VSS HI IN
D16 | -- | -- | -- | --
Location: Behind Left Side of I/P

#### Powertrain Control Module (PCM)-Automatic J4

Connector Part Information |

• | 12110244-J4

• | PNK

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A1 | -- | -- | -- | --
A2 | TAN/BLK | 422 | .50 | TCC OUT
A3 | DK BLU | 1530 | .50 | MPL OUT
A4 | -- | -- | -- | --
A5 | PPL | 898 | .50 | 4TH OUT
A6 | YEL/BLK | 1223 | .50 | 3RD OUT
A7 | LT GRN | 1222 | .50 | 2ND OUT
A8-A9 | -- | -- | -- | --
A10 | BLK/WHT | 451F | .35 | GROUND
A11 | BLK | 452T | .35 | TRANS FLUID TEMP SENSOR RTN
A12 | -- | -- | -- | --
B1 | -- | -- | -- | --
B2 | GRA | 773 | .50 | SEL SW B2
B3 | YEL | 772 | .50 | SEL SW B1
B4 | BLK/WHT | 771 | .50 | SEL SW B0
B5 | WHT | 776 | .50 | SEL SW B3
B6-B7 | -- | -- | -- | --
B8 | ORN/BLK | 586 | .35 | TRANS FLUID TEMP SENSOR IN
B9 | TAN/WHT | 551B | .80 | GROUND
B10 | RED/BLK | 1230 | .35 | TURBINE SHAFT SPEED SENSOR HI IN
B11 | DK BLU/WHT | 1231 | .35 | TURBINE SHAFT SPEED SENSOR LO IN
B12 | -- | -- | -- | --
Location: Behind Left Side of I/P

#### Starter Relay

Connector Part Information |

• | 12110541

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A1 | YEL/BLK | 625 | .35 | STARTER RELAY CONTROL
A2 | YEL | 575-AUTO 575A-MAN | 5.0 | SWITCHED CRANK FEED TO STARTER SOLENOID
B1-B2 | -- | -- | -- | --
C1 | YEL | 55A | 2.0 | CRANK FEED FROM IGNITION SWITCH
C2 | YEL | 5A | 2.0 | CRANK FEED FROM IGNITION SWITCH
Location: Taped to I/P Harness Forward of I/P Cluster

#### Throttle Position Sensor (TPS)

Connector Part Information |

• | 12129946

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK | 452J-AUTO 452M-MAN | .35 | TPS RTN AT PCM
B | DK BLU | 417A | .35 | TPS IN AT PCM
C | GRA | 474 | .35 | 5 V BATT
Location Engine Compartment-Center Rear