For 1990-2009 cars

### Removal Procedure

1. Open the sunroof.
2. Remove the locator block fastening screws.
3. Remove the locator block using the needle-nose pliers.

### Installation Procedure

1. Apply the Loctite 242® threadlocker, or equivalent, to the screws. Ensure that the last few threads are covered.
2. Install the locator blocks.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the locator block fastening screws.

Tighten
Tighten the sunroof locator blocks-to-sunroof module fasteners to 2 N·m (18 lb in).