For 1990-2009 cars

Application | Specifications
--- | ---
Torque Spec Description | Metric | English
ABS Wheel Speed Sensor | 8 | 53 lb in
Air Box Fasteners | 10 | 89 lb in
Ball Joint Stud Castle Nut | 75 | 55 lb ft
Battery Hold Down Fasteners | 9 | 80 lb in
Battery Terminal Bolts | 17 | 13 lb ft
Caliper Mount Bracket-to-Steering Knuckle | 110 | 81 lb ft
Electronic Variable Orifice (EVO) Actuator | 62 | 46 lb ft
Inner Tie Rod-to-Steering Gear | 95 | 70 lb ft
Intermediate Steering Shaft Cover-to-Body | 10 | 89 lb in
Intermediate Steering Shaft-to-Column Pinch Bolt | 47 | 35 lb ft
Intermediate Steering Shaft-to-Steering Gear Pinch Bolt | 47 | 35 lb ft
Left Brake Pipe-to-Brake Hose | 19 | 14 lb ft
Power Steering Hoses-to-Steering Gear | 27.5 | 20 lb ft
Power Steering Hoses-to-Steering Pump | 27.5 | 20 lb ft
Power Steering Pump-to-Bracket Bolt | 30 | 22 lb ft
Roll Connector Fasteners | 4 | 35 lb in
Steering Column Filler Panel Screws | 3 | 26 lb in
Steering Column Shroud Fasteners | 1.5 | 13 lb in
Steering Column Support Bolt (Lower) | 25 | 19 lb ft
Steering Column Support Bolt (Upper) | 35 | 26 lb ft
Steering Gear Adjuster Plug | 12 | 9 lb ft
Steering Gear Lock Nut | 70 | 52 lb ft
Steering Gear-to-Frame Fasteners | 50 | 37 lb ft
Steering Knuckle-to-Strut Fastener | 170 | 126 lb ft
Steering Wheel Attachment Nut | 35 | 26 lb ft
Steering Wheel Shroud-to-Steering Wheel Fasteners | 3 | 27 lb in
Tie Rod Linkage Installer | 45 | 33 lb ft
Tie Rod Lock Nuts | 70 | 35 lb ft
Tie Rod-to-Steering Knuckle Nut | 25 + 134° | 19 + 134° lb ft