For 1990-2009 cars

# Warranty Admin - July 1999 Labor Time Guide Updates

Subject: | Warranty Administration -- July, 1999 Labor Time Guide Updates

Models: | 1994-2000 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

Important: Please retain any changes made to the A, B, D and L Car Labor Time Guides as these vehicles have been discontinued since 1997 and the Labor Time Guides will not be republished. Changes to the P/H Truck Chassis should also be retained. The vehicle was discontinued in December, 1998. Please note: Labor Time Guides for these discontinued vehicles will not be republished.

#### LTG Update - C/K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
TRANSFER CASE ASSEMBLY - R&R |  | K4400 |  |  |  |  |  |  |
REMOVE AND REINSTALL |  |  |  |  |  |  |  |  |
243 |  |  | 2.1 | 2.1 | 2.1 | 2.1 | 2.1 | 2.1 | 2.1
236, 241 |  |  | 2.1 | 2.1 | 2.1 | 2.1 | 2.1 | 2.1 | 2.1
4401, 4470 |  |  | 2.1 | 2.1 | 2.1 | 2.1 | 2.1 | 2.1 | 2.1
246 | R |  | -- | -- | -- | 2.1 | 2.1 | 2.1 | 2.1
ADD:

- A- W/Skid Plate

0.2

0.2

0.2

0.2

0.2

0.2

0.2

B- To Recondtion Transfer Case Assy |  |  |  |  |  |  |  |  |
243 |  |  | 1.9 | 1.9 | 1.9 | 1.9 | 1.9 | 1.9 | 1.9
236, 241 |  |  | 1.9 | 1.9 | 1.9 | 1.9 | 1.9 | 1.9 | 1.9
4401, 4470 |  |  | 2.1 | 2.1 | 2.1 | 2.1 | 2.1 | 2.1 | 2.1
246 | R |  | -- | -- | -- | 3.0 | 3.0 | 3.0 | 3.0
PRE-DELIVERY INSPECTION - BASE TIME |  | Z7000 |  |  |  |  |  |  |
PICKUP |  |  | -- | -- | 1.2 | 1.2 | 1.2 | 1.2 | 1.2
SUBURBAN |  |  | -- | -- | 1.4 | 1.4 | 1.4 | 1.4 | 1.4
YUKON/TAHOE |  |  | -- | -- | 1.4 | 1.4 | 1.4 | 1.4 | 1.4
DENALI |  |  | -- | -- | -- | -- | -- | 2.0 | 2.0
INC: Installation of roof luggage carrier and running boards |  |  |  |  |  |  |  |  |
ESCALADE | R |  | -- | -- | -- | -- | -- | 3.5 | 2.0
INC: Installation of roof luggage carrier and running boards | R |  |  |  |  |  |  |  |
INC: OnStar VS-3B installation for 1999 only | R |  |  |  |  |  |  |  |
CAB/CHASSIS |  |  | -- | -- | 1.2 | 1.2 | 1.2 | 1.2 | 1.2
No Change to "ADD" Conditions |  |  |  |  |  |  |  |  |
*IND: N - New/R - Revised

#### LTG Update - C/K Platform - New Body Style

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
BELT, SAFETY FRONT (RETRACTOR SIDE) - R&R OR REPLACE

- PART GP: 14.875

RIGHT | R | C9040 | -- | -- | -- | -- | -- | 1.0 | 1.0
LEFT | R | C9041 | -- | -- | -- | -- | -- | 1.0 | 1.0
TOE, FRONT - ADJUST |  | E2000 |  |  |  |  |  |  |
C TRUCK | R |  | -- | -- | -- | -- | -- | 0.9 | 0.9
K TRUCK |  |  | -- | -- | -- | -- | -- | 0.5 | 0.5
HOUSING AND/OR GASKET, REAR MAIN SEAL - REPLACE |  | J1080 |  |  |  |  |  |  |
No Change to "PART GP" or "INC"

- NOTE: Applies to Engine Code V, T, U

MANUAL TRANS |  |  |  |  |  |  |  |  |
C TRUCK |  |  | -- | -- | -- | -- | -- | 3.3 | 3.3
K TRUCK |  |  | -- | -- | -- | -- | -- | 4.1 | 4.1
AUTO TRANS |  |  |  |  |  |  |  |  |
C TRUCK |  |  | -- | -- | -- | -- | -- | 3.5 | 3.5
K TRUCK | R |  | -- | -- | -- | -- | -- | 5.6 | 5.6
ADD:

- A- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers If Nec

R

--

--

--

--

--

0.3

0.3

SEAL(S), CRANKSHAFT REAR MAIN - REPLACE

- PART GP: 0.137

- INC: R&R trans

J1120

MANUAL TRANS |  |  |  |  |  |  |  |  |
C TRUCK |  |  | -- | -- | -- | -- | -- | 2.2 | 2.2
K TRUCK |  |  | -- | -- | -- | -- | -- | 3.7 | 3.7
AUTO TRANS |  |  |  |  |  |  |  |  |
C TRUCK |  |  | -- | -- | -- | -- | -- | 3.2 | 3.2
K TRUCK | R |  | -- | -- | -- | -- | -- | 3.9 | 3.9
*IND: N - New/R - Revised

#### LTG Update - G Van Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96-F | 96-1 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | T | V | W | X | Y
SENSOR, CRANKSHAFT POSITION - REPLACE

- POLICY: E

J4355

GAS |  |  | 0.3 | 0.3 | 0.3 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
DIESEL | R |  | 1.1 | 1.1 | 1.1 | 1.1 | 1.1 | 1.1 | 1.1 | 1.1
No Change to "ADD" Condition |  |  |  |  |  |  |  |  |  |
PUMP, FUEL INJECTION (DIESEL) - REPLACE

- PART GP: 3.280

- No Change to "POLICY" or "NOTE"

- No Change to "ADD" Conditions

R

J5955

3.6

3.6

3.6

5.2

5.2

5.2

5.2

5.2

*IND: N - New/R - Revised

#### LTG Update - J Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
CONTAINER AND CAP, WASHER FLUID - REPLACE

- PART GP: 10.154

- INC: Transfer washer pump as nec

WINDSHIELD | R | N3750 | 0.9 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0
*IND: N - New/R - Revised

#### LTG Update - J/E Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
SENSOR, CRANKSHAFT POSITION

- PART GP: 2.383

R

J4355

4WD |  |  | -- | -- | 0.2 | 0.2 | 0.2 | 4.3 | 4.3
2WD |  |  | -- | -- | 0.2 | 0.2 | 0.2 | 3.2 | 3.2
ADD: A- W/Skid Plate |  |  | -- | -- | 0.1 | 0.1 | 0.1 | 0.2 | 0.2
B- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis |  |  | -- | -- | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3
*IND: N - New/R - Revised

#### LTG Update - Medium Duty Platform

OPERATION | IND* | OP NUM | CAB STYLE YEAR VIN CODE
--- | --- | --- | ---
B | A/W5 | C | H
FOR 4.8L L-4 DIESEL CODE 4, 5 LABOR OPERATIONS, PLEASE USE ENGINE SECTION 3.9L L-4 DIESEL CODE H, K |  |  |  | -- | -- | --
NOTE: This Change Applies Only to 1999, 2000 Cab Style B |  |  |  |  |  |
*IND: N - New/R - Revised

#### LTG Update - S/T Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
PUMP, SECONDARY AIR INJECTION - REPLACE | N | J6050 | -- | -- | -- | -- | 0.7 | 0.7 | 0.7
BRACKET, SECONDARY AIR INJECTION PUMP - REPLACE | N | J6057 | -- | -- | -- | -- | 0.7 | 0.7 | 0.7
VALVE, SAI CHECK - REPLACE |  |  |  |  |  |  |  |  |
RIGHT | N | J6090 | -- | -- | -- | -- | 0.2 | 0.2 | 0.2
LEFT | N | J6091 | -- | -- | -- | -- | 0.3 | 0.3 | 0.3
SOLENOID, SAI VACUUM CONTROL - REPLACE | N | J6096 | -- | -- | -- | -- | 0.4 | 0.4 | 0.4
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

--

0-0.3

0-0.3

0-0.3

HOSE, SAI - REPLACE | N | J6120 | -- | -- | -- | -- | 0.9 | 0.9 | 0.9
PIPE, SAI - REPLACE

- PART GP: 3.675

- POLICY: E

CHECK VALVE TO RIGHT EXHAUST MANIFOLD | N | J6133 | -- | -- | -- | -- | 0.3 | 0.3 | 0.3
CHECK VALVE TO LEFT EXHAUST MANIFOLD | N | J6134 | -- | -- | -- | -- | 0.4 | 0.4 | 0.4
*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
REGULATOR, FRONT DOOR WINDOW - R&R OR REPLACE

- PART GP: 10.783

- No Change to "INCs" or "NOTE"

RIGHT MANUAL |  | C0180 | 0.8 | 0.8 | 0.8 | 0.8 |  |  |
LEFT MANUAL |  | C0181 | 0.8 | 0.8 | 0.8 | 0.8 |  |  |
RIGHT POWER |  | C0182 |  |  |  |  |  |  |
CHEVROLET |  |  | 0.8 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0
PONTIAC |  |  | 1.1 | 1.1 | 1.1 | 0.7 | 0.7 | 0.7 | 0.7
OLDSMOBILE |  |  | 1.1 | 1.1 | 1.1 | 1.1 | 0.7 | 0.7 | 0.7
BUICK |  |  | 1.1 | 1.1 | 1.1 | 0.7 | 0.7 | 0.7 | 0.7
LEFT POWER |  | C0183 |  |  |  |  |  |  |
CHEVROLET |  |  | 0.8 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0
PONTIAC |  |  | 1.1 | 1.1 | 1.1 | 0.7 | 0.7 | 0.7 | 0.7
OLDSMOBILE |  |  | 1.1 | 1.1 | 1.1 | 1.1 | 0.7 | 0.7 | 0.7
BUICK |  |  | 1.1 | 1.1 | 1.1 | 0.7 | 0.7 | 0.7 | 0.7
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

R

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised