For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Door Alignment Cone Nut | 10 N·m | 89 lb in
Door Check Link-to-Body Bolt | 10 N·m | 89 lb in
Door Check Link-to-Door Bolt | 25 N·m | 19 lb ft
Door Hinge-to-Body Bolts | 30 N·m | 22 lb ft
Door Hinge-to-Door Bolts | 30 N·m | 22 lb ft
Door Latch-to-Door Fasteners | 11 N·m | 98 lb in
Door Rear Applique | 2 N·m | 18 lb in
Door Striker Front Bolts | 25 N·m | 18 lb ft
Front Door Inside Release Handle Fasteners | 2.5 N·m | 22 lb in
Front Door Striker Bolts | 25 N·m | 18 lb ft
Inside Door Handle Screw (Sedan/Wagon) | 2.5 N·m | 22 lb in
Inside Rear Handle Screws (Coupe) | 5 N·m | 44 lb in
Manual Mirror Cable-to-Trim Panel Set Screw | 3 N·m | 27 lb in
Outer Door Panel Fasteners (Use Threadlocker) | 6 N·m | 53 lb in
Outer Sealing Strip-Belt Seal (Sedan/Wagon) | 6 N·m | 53 lb in
Outside Rear View Mirror Nuts | 10 N·m | 89 lb in
Power Mirror Motor Screws | 3 N·m | 27 lb in
Rear Door Check Link-to-Body Bolt | 25 N·m | 19 lb ft
Rear Door Check Link-to-Door Nuts | 10 N·m | 89 lb in
Rear Door Exterior Panel Fasteners (3-Door Coupe) (Front of Door) | 7-11 N·m | 80 lb in
Rear Door Exterior Panel Fasteners (3-Door Coupe) (Rear of Door) | 5-7 N·m | 53 lb in
Rear Door Front Applique Screws (Sedan/Wagon) | 2 N·m | 18 lb in
Rear Door Front Window Guide Bolt (Sedan/Wagon) | 7.5 N·m | 67 lb in
Rear Door Hinge Check Link-to-Body Bolts | 16 N·m | 12 lb ft
Rear Door Hinge-to-Body Bolts (Coupe) | 28 N·m | 21 lb ft
Rear Door Hinge-to-Body Bolts (Sedan/Wagon) | 30 N·m | 22 lb ft
Rear Door Hinge-to-Door Bolts (Coupe) | 28 N·m | 21 lb ft
Rear Door Hinge-to-Door Bolts (Sedan/Wagon) | 30 N·m | 22 lb ft
Rear Door Inside Release Handle Fastener | 2.5 N·m | 22 lb in
Rear Door Latch Fasteners (Sedan/Wagon) | 11 N·m | 97 lb in
Rear Door Lower Latch Bolts (Coupe) | 24 N·m | 18 lb ft
Rear Door Lower Striker-to-Body Bolts (Coupe) | 25 N·m | 18 lb ft
Rear Door Outer Sealing Strip-Belt Seal | 2 N·m | 18 lb in
Rear Door Quarter Window Retaining Bolts (Coupe) | 2 N·m | 18 lb in
Rear Door Rear Window Guide Bolts (Sedan/Wagon) | 7.5 N·m | 67 lb in
Rear Door Release Handle Fasteners (Coupe) | 2.5 N·m | 23 lb in
Rear Door Stabilizer Pin (Sedan/Wagon) | 30 N·m | 22 lb ft
Rear Door Striker Fasteners | 25 N·m | 19 lb ft
Rear Door-to-Body Bolts (Coupe) | 28 N·m | 21 lb ft
Rear Door Trim Panel Fasteners (Coupe) | 5 N·m | 44 lb in
Rear Door Upper Hinge Check Link Bolts | 11 N·m | 8 lb ft
Rear Door Upper Latch Bolts (Coupe) | 24 N·m | 18 lb ft
Rear Door Upper Striker-to-Body Bolts (Coupe) | 32 N·m | 24 lb ft
Rear Outer Door Panel Bolts (Use Threadlocker) | 6 N·m | 53 lb in
Rear Side Door Release Handle Fasteners (Coupe) | 2.5 N·m | 23 lb in