For 1990-2009 cars

### Lining Inspection

Inspect the brake linings at 10 000 km (6,000 miles), then every 20 000 km (12,000 miles), and any time that the wheels are removed (tire rotation, etc.). Check both ends of the outer pad by looking in at each end of the caliper. These are the points at which the highest rate of wear normally occurs. However, at the same time, check the lining thickness on the inner shoe to make sure that it has not worn prematurely. Look down through the inspection hole in the top of the caliper to view the inner shoe. Whenever the thickness of any lining is worn to 2.0 mm (0.08 in) or less, at either end of the shoe, all disc brake linings should be replaced at the same time.

### Lining Replacement

Saturn replacement brake lining material is recommended to maintain the balance between front and rear brake performance. Saturn replacement brake parts have been carefully selected to provide proper brake balance for purposes of both stopping distance, and control over a full range of operating conditions. Installation of front or rear brake lining material other than Saturn replacement parts, can change the intended brake balance of the vehicle.

When installing new front brake pads or when servicing front disc brakes, remove all rust and corrosion from the caliper brackets and the spring clips. If reinstalling used brake pads, remove all rust and corrosion from the ends of the brake pads and from the notch. Make sure the brake pads move freely in the caliper brackets when the brakes are assembled.