For 1990-2009 cars

### Removal Procedure

1. Exert pressure on the rear of the power window/mirror switch with hand.
2. Using a small flat bladed screwdriver, carefully lift the switch at the rear retainer assembly tabs.
3. Lift the switch from console.
4. Disconnect the electrical connectors by locating the retention tabs and disengaging the connectors.

### Installation Procedure

1. Connect the power window/mirror switch assembly electrical connectors.
2. Install the power window/mirror switch assembly.
3. Check the operation of all the switches.