For 1990-2009 cars

### Road Test

Use the flow chart on the facing page to determine if a vehicle pull is most likely caused by steering pull or torque steer. Perform the road test on a flat level road and with minimum wind conditions.

Drive - Steady Speed: 72-88 km/h (45-55 mph) in drive maintaining a steady speed

Neutral - Coast: 72-88 km/h (45-55 mph) in neutral coasting

### Front Wheel Drive Steering Pull Correction Chart

### Front Wheel Drive Torque Steer Correction Chart

### Front Wheel Drive Wander Correction Chart

### Vibration Complaint