For 1990-2009 cars

### Removal Procedure

1. Remove the shroud top vent grille. Refer to Air Inlet Grille Panel Replacement in Body Front End.
2. Disconnect the washer fluid hose from the vent grille.
3. Disconnect the washer fluid hose from the washer nozzle.
4. Pinch the attachment fingers on the bottom of the nozzle and remove the nozzle.

### Installation Procedure

1. Install the nozzle through the opening in the shroud top vent grille and push into place.

Important: Make sure that the nozzle is fully seated in the grille and the attachment fingers are in place.

2. Attach the washer fluid hose to the nozzles.
3. Attach the washer fluid hose to the vent grille.
4. Install the shroud top vent grille. Refer to Air Inlet Grille Panel Replacement in Body Front End.