For 1990-2009 cars

### Removal Procedure

Notice: Cut only deep enough to separate the crimp ring. Take care not to cut the pipe.

Important: When cutting crimp ring, cut at 30 degree angle to centerline of hose.

1. Use hacksaw to cut crimp ring.
2. Use a flat head screwdriver to separate and remove crimp ring from hose.
3. Remove heater hose from pipe.

### Installation Procedure

1. Install thermostat hose on pipe.
2. Install new clamp on hose. Position clamp at 11 o'clock.