For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
2. Lower the seat backs.
3. Remove the left and right body lock pillar lower trim moldings. Refer to Body Lock Pillar Trim Finish Molding Replacement - Lower .

Notice: It is not necessary to remove the shoulder belt. Remove lock pillar and place on floor with shoulder belt routed through opening. Care must be taken not to damage lock pillar or shoulder belt.

4. Remove the body lock pillar upper trim molding on one side only. Refer to Garnish Molding Replacement - Body Lock Pillar Upper .
5. Remove the child safety seat top tether anchor covers.
6. Slide the rear window trim finish panel out from under the remaining body lock pillar upper molding, over the top tether anchors and remove the panel from the vehicle.

### Installation Procedure

1. Slide the rear trim finish panel under the body lock pillar upper trim molding and over the top tether anchors.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rosebud attachment fasteners.
3. Install the body lock pillar upper trim molding. Refer to Garnish Molding Replacement - Body Lock Pillar Upper .
4. Install the body lock pillar lower molding. Refer to Body Lock Pillar Trim Finish Molding Replacement - Lower .
5. Install the child safety seat top tether anchor covers.
6. Raise the rear seat backs.
7. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.