For 1990-2009 cars

Action | Normal Results
--- | ---
Put the mirror select switch in LEFT position. Operate the mirror adjustment switch (pad) in up and down. | The left outside mirror should move up and down smoothly.
Operate the mirror adjustment switch (pad) in right and left. | The left outside mirror should move right and left smoothly.
Put the mirror select switch in RIGHT position: Operate the mirror adjustment switch (pad) in up and down. | The right outside mirror should move up and down smoothly.
Operate the mirror adjustment switch (pad) in right and left. | The right outside mirror should move right and left smoothly.