For 1990-2009 cars

### Removal Procedure

1. Straighten out the retaining tabs, release the front hook-and-loop retainer attachments and remove the trunk side wall trim.
2. Disengage the hook-and-loop retainer attaching the trunk floor carpet to the seat backs and remove the trunk floor carpet.

### Installation Procedure

1. Install the trunk side wall trim, engage the front hook-and-loop retainer attachments.
2. Slide the tabs through the trim panel and bend them over to secure the trim panel.
3. Install the trunk floor carpet and engage the trunk floor carpet hook-and-loop retainer with the seat backs.