For 1990-2009 cars

### Removal Procedure

1. Remove the trunk floor carpet and the tire board. Refer to Rear Compartment Floor Panel Carpet Replacement .
2. Remove the spare wheel and jack.
3. Lift the acoustic material and separate it from the floor at glued locations.

### Installation Procedure

1. Apply hot melt glue to the rear floor pan. Align the material to the floor at the jack bracket on the right side and install the rear floor acoustic material.
2. Install the trunk floor carpet. (Refer to Rear Compartment Floor Panel Carpet Replacement .