For 1990-2009 cars

### Removal Procedure

1. Remove the door panel. Refer to Front Side Door Trim Panel Replacement in Doors.
2. Remove the speaker fasteners and pull the speaker away from the door assembly.
3. Disconnect the speaker wire harness from the speaker.
4. Remove the speaker from the vehicle.

### Installation Procedure

1. Connect the speaker harness wire to the speaker.
2. Place the speaker in the door assembly and install the fasteners.
3. Install the door panel. Refer to Front Side Door Trim Panel Replacement in Doors.