For 1990-2009 cars

# Radio Displays XM Error or DTC U1137 - keywords communication digital loss nocomm operation performance tech2 U2K

Subject: | Radio Displays "XM error" or DTC U1137

Models: | All 2002-2006 XM Equipped Vehicles

The following diagnosis might be helpful if the vehicle exhibits the symptom(s) described in this PI.

### Condition/Concern:

The radio may display "XM error" and a possible U1137 DTC stored in the radio. The concern is due to the radio losing communication with the digital radio receiver while the key is on. The message is only displayed on the radio during the effected key cycle.

### Recommendation/Instructions:

Perform diagnostics for the loss of communication with the Digital radio receiver (DRR).

Please follow this diagnostic or repair process thoroughly and complete each step. If the condition exhibited is resolved without completing every step, the remaining steps do not need to be performed.