For 1990-2009 cars

## Rear Bumper Fascia Replacement Coupe

### Removal Procedure

1. Raise the rear compartment lid.
2. Remove the plastic retainers from the bumper filler.
3. Remove the plastic retainers, rear fascia bottom to bumper impact bar.
4. Remove the plastic retainers, wheelhouse liners to rear fascia.
5. Remove the fascia by sliding rearward, disengaging shoulder bolts and fascia to quarter panel sliding retainers.

### Installation Procedure

1. If installing a new rear fascia, transfer the wheeliner nuts, fascia brackets and bumper filler.
2. Install the fascia over the bumper impact bar. Engage the fascia ends (key slots) over the shoulder bolts extending down from the quarter panel and pushing the fascia forward to lock the fascia to the quarter panels.
3. Install the plastic retainers in wheelhouse liner to the fascia ends.
4. Install the plastic retainers, rear fascia bottom to the fascia support brackets.
5. Install the plastic retainers to the rear bumper filler.
6. Close the rear compartment lid.

## Rear Bumper Fascia Replacement Sedan

### Removal Procedure

1. Raise the rear compartment lid.
2. Remove the plastic retainers from the rear bumper filler.
3. Remove the plastic retainers, rear fascia bottom to fascia support brackets.
4. Remove the plastic retainers, wheelhouse liners to rear fascia.
5. Remove the fascia by sliding it rearward.
6. If replacing the fascia, transfer the following items:

• | Fascia brackets

• | Rear bumper filler

### Installation

1. Install the fascia over the bumper sub-assembly. Engage the fascia ends (key slots) over the shoulder bolts extending down from the quarter panel and pushing the fascia forward to lock the fascia to the quarter panels.
2. Install the plastic retainers in wheelhouse liner to fascia ends.
3. Install the plastic retainers, rear fascia bottom to the fascia support brackets.
4. Align the bumper filler and install the plastic retainers.
5. Close the rear compartment lid.

## Rear Bumper Fascia Replacement Wagon

### Removal Procedure

1. Raise the liftgate.
2. Remove the plastic retainers from the rear bumper filler.
3. Remove the rear bumper filler. Refer to Bumper Filler Replacement .
4. Remove the plastic retainers, rear fascia bottom to fascia support brackets.
5. Remove the pushpins, wheelhouse liners to rear fascia.
6. Remove the fascia by sliding it rearward.
7. If replacing fascia, transfer the following items:

• | Fascia brackets

• | Rear bumper filler

### Installation Procedure

1. Install the fascia over the bumper sub-assembly. Engage the fascia ends (key slots) over the shoulder bolts extending down from the quarter panel and pushing the fascia forward to lock the fascia to quarter panels.
2. Install the pushpins in wheelhouse liner to the fascia ends.
3. Install the plastic retainers, rear fascia bottom to the fascia support brackets.
4. Install rear bumper filler. Refer to Bumper Filler Replacement .
5. Align the bumper filler and install the plastic retainers.
6. Close the liftgate.