For 1990-2009 cars

Power mirror system provides ability to electrically position driver and passenger side mirror. The system consists of a switch mounted on driver's side door handle, and two reversible electric motors for each mirror.

### Power Mirror Switch

The power mirror switch controls the right and left mirror position. The mirror select switch (rocker switch) allows control of the right or left mirror. The mirror adjustment switch (pad switch) allows control of the mirror position: UP, DOWN, RIGHT, or LEFT.

With the mirror select switch in the LEFT mirror position, the circuit operation is as follows:

If the mirror adjustment switch is pressed in the UP position, battery voltage from circuit 340 is applied to circuit 889 to the up/down mirror motor in the left mirror. The mirror switch supplies a ground path for circuit 90 through the closed contacts to circuit 550, and the mirror moves up. When the mirror adjustment switch is pressed in the DOWN position, battery voltage from circuit 340 is applied through to circuit 90 to the up/down mirror motor in the left mirror. The mirror switch supplies a ground path for circuit 889 through the closed contacts to circuit 550, and the mirror moves down.

When the mirror adjustment switch is moved to the RIGHT position, battery voltage from circuit 340 is applied through to circuit 889 to the right/left mirror motor in the left mirror. The mirror switch supplies a ground path for circuit 90 through the closed contacts to circuit 550, and the mirror moves right. When the mirror adjustment switch is moved to the LEFT position, battery voltage from circuit 340 is applied through to circuit 90 to the right/left mirror motor in the left mirror. The mirror switch supplies a ground path for circuit 881 through the closed contacts to circuit 550, and the mirror moves left. The controls of the mirror position switch are the same for the right and left position of the mirror select switch.

With the mirror select switch in the RIGHT mirror position, the circuit operation is as follows:

If the mirror adjustment switch is pressed in the UP position, battery voltage form circuit 340 is applied to circuit 89 to the up/down mirror motor in the left mirror. The mirror switch supplies a ground path for circuit 82 through the closed contacts to circuit 550, and the mirror moves up. When the mirror adjustment switch is pressed in the DOWN position, battery voltage from circuit 340 is applied through to circuit 82 to the up/down mirror motor in the right mirror. The mirror switch supplies a ground path for circuit 89 through the closed contacts to circuit 550, and the mirror moves down.

When the mirror adjustment switch is moved to the RIGHT position, battery voltage from circuit 340 is applied through to circuit 81 to the right/left mirror motor in the right mirror. The mirror switch supplies a ground path for circuit 82 through the closed contacts to circuit 550, and the mirror moves right. When the mirror adjustment switch is moved to the LEFT position, battery voltage from circuit 340 is applied through to circuit 82 to the right/left mirror motor in the right mirror. The mirror switch supplies a ground path for circuit 81 through the closed contacts to circuit 550, and the mirror moves left. The controls of the mirror position switch are the same for the right and left position of the mirror select switch.

### Power Mirror Motors

Each mirror has two reversible electric motors: one to adjust mirror view up and down, the other to adjust right or left.