For 1990-2009 cars

### Removal Procedure

Caution: Ensure that the vehicle is properly supported and squarely positioned. To help avoid personal injury when a vehicle is on a hoist, provide additional support for the vehicle on the opposite end from which the components are being removed.

1. Raise the vehicle on a hoist.
2. Remove the trailing arm-to-knuckle fastening nut.
3. Remove the 2 trailing arm-to-body fasteners.
4. Slide the trailing arm from the knuckle.

### Installation Procedure

1. Install the ailing arm into the knuckle and hand tighten the fastener nut.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the trailing arm into the body and secure the trailing arm with fasteners.

Tighten
Tighten the trailing arm-to-body fasteners to 120 N·m (89 lb ft).

3. Secure the trailing arm-to-knuckle fastener.

Tighten
Tighten the trailing arm-to-knuckle fasteners to 100 N·m (74 lb ft).