For 1990-2009 cars

### Removal Procedure

1. Remove the clamp and hose from the coolant recovery reservoir.
2. Remove the hose from the hold down clips.
3. Remove the clamp and hose from the intake manifold.

### Installation Procedure

1. Cut the new hose to length from the bulk roll.
2. Install the hose and clamp on the intake manifold. Position the clamp at 10 o'clock.

Notice: Make sure the cooling system deaeration hose does not contact the cowl as it will cause a noise inside the vehicle. It may be necessary to shorten the hose.

3. Install the hose and clamp on the coolant surge tank. Position the clamp at 11 o'clock.