For 1990-2009 cars

## Body Lock Pillar Trim Finish Molding Replacement - Lower Sedan/Wagon

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
2. Remove the rear seat carpet retainer molding.
3. Lower the rear seat back.
4. Remove the body lock trim finish molding by pulling firmly, starting at the bottom of the molding to disengage the clips.
5. Slide the molding out from under the body lock pillar upper trim finish molding and the weatherstrip.

### Installation Procedure

1. Slide the body lock trim finish molding upper tab into the body lock pillar upper trim finish molding.
2. Line up the attaching clips and firmly snap the body lock trim finish molding into place.

Important: The outboard tabs of the body lock pillar trim finish molding must be positioned under the weatherstrip after installation.

3. Install the rear seat carpet retainer molding.
4. Raise the rear seat back assembly.
5. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.