For 1990-2009 cars

## Rear Compartment Lid Latch Replacement With Remote Keyless Entry

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable from the battery.
2. Open the lid.
3. Remove the 2 bolts holding the lid latch to the lid.
4. Disconnect the lock cylinder rod and the wiring clip.

### Installation Procedure

1. Connect the lock cylinder rod and the wiring clip.

Notice: Refer to Fastener Notice in the Preface section.

2. Position the lid latch to the compartment lid and install the lid latch with the 2 bolts.

Tighten
Tighten the rear compartment lid latch bolts to 10 N·m (89 lb in).

3. Close the lid.
4. Connect the negative battery cable to the battery.

## Rear Compartment Lid Latch Replacement Without Remote Keyless Entry

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the lock cylinder rod and the release cable from the latch.
3. Remove the screws, disconnect the cargo lamp harness, and remove the latch.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Connect the cargo lamp harness to the latch and install the latch with screws.

Tighten
Tighten the rear compartment lid latch bolts to 10 N·m (89 lb in).

2. Connect the release cable and lock the cylinder. Connect to the latch.
3. Connect the negative battery cable.