For 1990-2009 cars

### Removal Procedure

1. Remove the wiper module. Refer to Windshield Wiper Motor Replacement .
2. Disconnect the wiper control module electrical connector.
3. Using a thin bladed screwdriver, gently pry the center tabs of the wiper control module retainer arms.
4. Remove the wiper controller from the wiper module.

### Installation Procedure

1. Install the wiper controller to the wiper module.
2. Connect the wiper control module electrical connector.
3. Install the wiper module. Refer to Windshield Wiper Motor Replacement .