For 1990-2009 cars

### Removal Procedure

1. Cycle glass to full down position.
2. Lift rear end of inner sealing strip and carefully pull from inner belt flange by lifting up from rear to front. Use of a putty knife with the blade covered with tape may be needed to gently pry seal from the flange.

### Installation Procedure

1. Position inner belt sealing strip to door starting at the rear edge.
2. Press seal onto inner belt flange.