For 1990-2009 cars

Table 1: | Gear Teeth Counts and Ratios
Table 2: | Clutch, Clutch Controls, and Flywheel Specifications
Table 3: | Blocker Ring Clearance Specifications
Table 4: | Axial Play Specifications

#### Gear Teeth Counts and Ratios

Application | 2000/2001 MP2 (Base) Gear Teeth Count | 2000/2001 MP3 (Performance) Gear Teeth Count
--- | --- | ---
1st Drive | 12 | 12
1st Driven | 39 | 39
2nd Drive | 20 | 20
2nd Driven | 39 | 39
3rd Drive | 29 | 26
3rd Driven | 34 | 37
4th Drive | 37 | 31
4th Driven | 30 | 32
5th Drive | 43 | 37
5th Driven | 26 | 27
Reverse Drive | 13 | 13
Reverse Idler | 31 | 31
Reverse Driven | 38 | 38
Output Shaft | 16 | 16
Ring Gear | 65 | 65
All SOHC engines use MP2 transaxle, and all DOHC engines use MP3 transaxle.

Application | Gear Ratio | Gear Ratio
--- | --- | ---
1st Gear | 3.250 | 3.250
2nd Gear | 1.95 | 1.95
3rd Gear | 1.172 | 1.423
4th Gear | 0.811 | 1.033
5th Gear | 0.605 | 0.730
Reverse Gear | 2.923 | 2.923
Final Drive Ratio | 4.063 | 4.063

### Gear Identification

All MP3 unique gears have an identification groove on the outer diameter of the gear teeth. There is no identification mark on MP2 unique gears, or MP2 and MP3 common gears.

#### Clutch, Clutch Controls, and Flywheel Specifications

Measurement | Specification
--- | ---
Metric | English
Clutch Disc Thickness

- Standard
- Service Limit

5.2-7.3 mm

5.2 mm

0.205-0.287 in

0.205 in

Flywheel
Thickness

- Standard
- Service Limit

28.25 mm

28.25 mm

1.11 in

1.11 in

Runout

- Standard
- Service Limit

0.15 mm

0.15 mm

0.006 in

0.006 in

Warpage

- Standard
- Service Limit

0.15 mm

0.15 mm

0.006 in

0.006 in

Pressure Plate Warpage

- Standard
- Service Limit

0.15 mm

0.15 mm

0.006 in

0.006 in

Clutch Controls Clutch Pedal Travel

- Standard
- Service Limit

127-140 mm

127 mm

5.00-5.50 in

5.00 in

#### Blocker Ring Clearance Specifications

Application | Metric | English
--- | --- | ---
Blocker Ring Clearance* | 0.4 mm | 0.020 in
*Measurements are the same for Standard and Service Limit

#### Axial Play Specifications

Measurement | Specification
--- | ---
Metric | English
Between 1st Driven Gear and 1st Driven Gear Thrust Washer

- Standard
- Service Limit

0.20-0.496 mm

0.496 mm

0.008-0.019 in

0.019 in

Between 2nd Driven Gear and 3rd/4th Cluster Gear

- Standard
- Service Limit

0.20-0.35 mm

0.35 mm

0.008-0.014 in

0.014 in

Between 3rd Drive gear and Input Shaft

- Standard
- Service Limit

0.20-0.35 mm

0.35 mm

0.008-0.014 in

0.014 in

Between 4th Drive Gear and 4th Gear Thrust Washer

- Standard
- Service Limit

0.20-0.35 mm

0.35 mm

0.008-0.014 in

0.014 in

Between 5th Drive gear and 5th Gear Thrust Washer

- Standard
- Service Limit

0.20-0.35 mm

0.35 mm

0.008-0.014 in

0.014 in