For 1990-2009 cars

### Removal Procedure

1. Disengage the manual window regulator handle retention spring with a standard handle tool, or by working a cloth back and forth between the handle and the bearing plate.
2. Remove the handle and bearing plate.

### Installation Procedure

1. Install the window regulator handle retention spring on the handle.
2. Install the bearing plate.
3. Install the handle in a forward and slightly up position with the window in a closed position.