For 1990-2009 cars

### Removal Procedure

1. Power the sunroof to the vent position.
2. Remove the 6 screws attaching the sunroof glass to the module, and remove the glass.

### Installation Procedure

1. Set the glass in position on the sunroof module.
2. Apply Loctite Small Screw Threadlocker 222®, or equivalent, to the sunroof glass attaching screws and install.
3. With the sunroof in the closed position, adjust the glass to 1 mm (0.040 in) below the surface of the roof at the front, and 1 mm (0.040 in) above the roof surface at the rear.

Notice: Refer to Fastener Notice in the Preface section.

4. Tighten the bolts.

Tighten
Tighten the sunroof glass-to-sunroof bolts to 3 N·m (27 lb in).