For 1990-2009 cars

The ABS enable relay is inside the ABS control module (EBTCM) and provides shut-down capability in the event of a system failure.

### DTC Parameters

DTC C0124 will set if:

• | Enable relay is stuck on when commanded Off.

• | ABS and dynamic rear proportioning (DRP) will be fully functional.

• | The wrench light will be turned On.

### Diagnostic Aids

The ABS Control Module must be replaced.