For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Console Arm Rest Fasteners | 1.5 N·m | 13 lb in
Console Front Fasteners | 2.2 N·m | 19 lb in
Console Latch Fastener | 1.5 N·m | 13 lb in
Console Rear Fastener | 2.2 N·m | 19 lb in
Endcap-to-I/P Fasteners | 2.2 N·m | 19 lb in
Glove Compartment Door Outer Cover Fastener | 2.2 N·m | 19 lb in
Glove Compartment Latch Fastener | 2 N·m | 18 lb in
Ground Wire-to-H-Brace | 2 N·m | 18 lb in
H-Brace-to-Floor Panel Bolts | 25 N·m | 19 lb ft
HVAC Control Head-to-I/P Fasteners | 2.5 N·m | 22 lb in
Hood Release Lever-to-I/P Filler Panel Fastener | 1.5 N·m | 13 lb in
I/P Cluster-to-I/P Housing Fasteners | 2.2 N·m | 19 lb in
I/P Endcap-to-I/P Fasteners | 2.2 N·m | 19 lb in
I/P Endcap-to-I/P Housing Fasteners | 2.2 N·m | 19 lb in
I/P Retainer Assembly Bolts | 10 N·m | 89 lb in
I/P Upper Trim Panel Fasteners | 6 N·m | 53 lb in
Passenger Side Inflator Module Bolts | 10 N·m | 89 lb in
Passenger Side Inflator Module Cover Fasteners | 2.2 N·m | 19 lb in
Radio Ground Strap-to-H-Brace | 2.2 N·m | 19 lb in
Radio-to-I/P Fasteners | 2.5 N·m | 22 lb in
Steering Column Filler Panel Fasteners | 2.2 N·m | 19 lb in
Steering Column Shroud Fasteners | 1.5 N·m | 13 lb in
Steering Column-to-I/P Bolts | 35 N·m | 26 lb ft