For 1990-2009 cars

# Hesitation or Stumble During Tip-In Launch After Spark Plug Wires Were Reinstalled or Replaced - kw 1.9 L24 LL0 SOHC DOHC accelerate throttle

Subject: | Hesitation or Stumble during Tip-In Launch after Spark Plug Wres Were Reinstalled or Replaced

Models: | .

The following diagnosis might be helpful if the vehicle exhibits the symptom described in the PI.

### Condition/Concern:

Hesitation or stumble during tip-in launch after spark plug wires were reinstalled or replaced in 91-02 DOHC (LL0) or 95-02 SOHC (L24), 1.9L engines.

### Recommendation/Instructions:

The #1 and #4 spark plug wires are connected to the incorrect coil towers. Connect the #1 spark plug wire to the #1 coil tower and the #4 spark plug wire to the #4 coil tower.

.

Please follow this diagnosis process thoroughly and complete each step. If the condition exhibited is resolved without completing every step, the remaining steps do not need to be performed. If these steps do not resolve the condition, please contact GM TAC for further diagnostic assistance.

### Models:

(91-02 Saturn S-Series 1.9L DOHC (LLO)) and (95-02 Saturn S-Series 1.9L SOHC (L24))

.