For 1990-2009 cars

### Removal Procedure

1. Remove outer belt seal end cap screw.

Important: A putty knife with the blade covered with tape may be needed to gently pry belt seal from flange.

2. Starting at front, lift outer belt seal.

### Installation Procedure

1. Press outer belt seal onto outer belt flange.
2. Check alignment at front edge of door.

Notice: Refer to Fastener Notice in the Preface section.

3. Install and tighten outer belt seal end cap.

Tighten
Tighten the rear door outer-sealing strip belt seal to 2 N·m (18 lb in).