For 1990-2009 cars

## Striker Cover Replacement Coupe - 2nd Design

### Removal Procedure

1. Disengage the push pins by pushing the center pin with an awl.
2. Slide the striker cover outward to remove it from the seat belt bezel tabs.

### Installation Procedure

1. Slide the striker cover inboard until the striker tabs rest on the seat belt bezel ledge.
2. Push the center pin back through the push pin so that it protrudes above the head of the push pin.
3. Place the push pins in the striker holes and push the center pin until it is flush with the push pin head to engage.