For 1990-2009 cars

### Removal Procedure

1. Remove the seat from the vehicle. Refer to Front Seat Replacement - Bucket .
2. Remove the recliner handle.
3. Remove the seat adjuster side cover.
4. Disengage the seat back cover J-strip at the bottom of the seat cover.
5. Remove the bolts and remove the seat cushion/cover assembly.
6. Disengage all the seat cover J-strips. Remove the cushion/cover assembly from the frame.

### Installation Procedure

1. Install the cushion/cover assembly over the seat frame. Engage all the seat cover J-strips to the seat frame except the rear.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the seat cushion assembly to the adjusters.

Tighten
Tighten the front seat adjuster-to-seat bolts to 27 N·m (20 lb ft).

3. Wrap the seat cushion cover rear flap to cover up the recliner cross tube and engage the seat cushion cover rear J-strip to seat cushion frame. Refer to the following:

• | Seat Cover (1)

• | Cushion Frame (2)

• | Foam Pad (3)

• | Cross Tube (4)

• | Seat Cover J-Strip (5)

4. Install the seat adjuster side cover.

Tighten
Tighten the seat side cover fasteners to 2.5 N·m (22 lb in).

5. Install the recliner handle.

Tighten
Tighten the recliner handle fastener to 3 N·m (27 lb in).

6. Install the seat into the vehicle. Refer to Front Seat Replacement - Bucket .