For 1990-2009 cars

### Removal Procedure

1. Lower door window.
2. Remove inner sealing strip (belt seal).
3. Lift one end of secondary weatherstrip.
4. Carefully pull secondary weatherstrip from door frame.

### Installation Procedure

1. Starting at mirror patch, install the front weatherstrip locating notch and work weatherstrip toward rear upper corner.
2. Install rear weatherstrip locating notch at the belt line.
3. Install inner sealing strip (belt seal).