For 1990-2009 cars

### Removal Procedure

1. Remove accessory drive belt and power steering pump pulley.
2. Remove shield retaining bolts.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install new shield with attaching bolts.

Tighten
Tighten the accessory drive belt shield bolts to 8 N·m (70 lb in).

2. Install power steering pump pulley and accessory drive belt.

Tighten
Tighten the belt tensioner pulley to 30 N·m (22 lb ft).