For 1990-2009 cars

## Rear Bumper Impact Bar Replacement Sedan/Wagon

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Impact Bar Replacement .
2. Remove the lower attaching bolts from the outside.
3. Remove the upper attaching nuts from inside the rear compartments.
4. Remove the impact bar.

### Installation Procedure

Important: If reusing the bumper impact bar after a rear-end collision, inspect bar for damage. If the bar is not torn or cracked and retains its shape, it can be reused.

1. Position the impact bar to rear end structure.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the attaching nuts and bolts.

Tighten
Tighten the bolts to 30 N·m (22 lb ft).

3. Install the fascia. Refer to Rear Bumper Fascia Replacement .

## Rear Bumper Impact Bar Replacement Coupe

### Removal Procedure

1. Remove the rear fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the lower attaching bolts from the outside.
3. Remove the upper attaching nuts from inside the rear compartment.

### Installation

Important: If reusing the bumper impact bar after a rear-end collision, inspect the bar for damage. If the bar is not torn or cracked and retains its shape, it can be reused.

1. Position the impact bar to rear end structure.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the attaching nuts and bolts.

Tighten
Tighten the bolts to 25 N·m (19 lb ft).

3. Install the fascia. Refer to Rear Bumper Fascia Replacement .