For 1990-2009 cars

## Bumper Filler Replacement Wagon

### Removal Procedure

1. Open the wagon liftgate.
2. Remove the pushpins from the front of the rear bumper filler.
3. Lift the front of the rear bumper filler, slide it forward of the rear fascia and lift it off.

### Installation procedure

1. Align the tabs in the rear bumper filler to the slots in the rear fascia. Insert the tabs into slots.
2. Slide the rear bumper fascia rearward until the tabs are locked into place.
3. Install the pushpins in the front of the rear bumper filler.
4. Close the liftgate.