For 1990-2009 cars

## Front Bumper Fascia Energy Absorber Replacement Sedan/Wagon

### Removal Procedure

1. Remove the front bumper impact bar. Refer to Front Bumper Impact Bar Replacement .
2. Remove the plastic fasteners that retain the absorber to the impact bar.

### Installation Procedure

1. Position the energy absorber to the bumper impact bar; attach it with a plastic fastener.
2. Install front bumper impact bar. Refer to Front Bumper Impact Bar Replacement .

## Front Bumper Fascia Energy Absorber Replacement Coupe

### Removal Procedure

1. Remove the front bumper impact bar. Refer to Front Bumper Impact Bar Replacement .
2. Remove the plastic fasteners that retain the absorber to the impact bar.

### Installation Procedure

1. Position the energy absorber to the bumper impact bar, attach it with plastic fastener.
2. Install the front bumper impact bar. Refer to Front Bumper Impact Bar Replacement .