INFO ON SERVICE REPLACEMENT WINDSHIELD-REMOVE SPACER BLOCK. Saturn Saturn 1991

For 1990-2009 cars

# INFO ON SERVICE REPLACEMENT WINDSHIELD-REMOVE SPACER BLOCK

#### SUBJECT: Information on Service Replacement Windshield

Due to the addition of "MODELS AFFECTED" with a VIN breakpoint, this bulletin supersedes bulletin 91 - T - 02, which should be discarded.

#### MODELS AFFECTED: 1991 Saturn SL, SL1, and SL2 Sedans built before vehicle identification number (VIN) MZ112000.

PURPOSE: Removal of spacer blocks when installing a replacement windshield.

PROCEDURE: When replacing windshields on some early model SL, SL1 or SL2 vehicles, the three spacer blocks, located at the bottom of the windshield area (refer to figure), must be removed from the vehicle and discarded. When installing a replacement windshield, check to see if spacer blocks are attached to the bottom of the windshield. If spacer blocks are attached, remove blocks before installing the windshield on the vehicle.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.