Power Door Lock Actuators Chatter When Activated from the Drivers Door Key Cylinder Switch. Saturn Saturn 1991

For 1990-2009 cars

# Power Door Lock Actuators Chatter When Activated from the Drivers Door Key Cylinder Switch

Subject: | Power Door Lock Actuators Chatter When Activated from the Driver's Door Key Cylinder Switch (Recode Lock Cylinders)

Models: | All 1991 Saturns w/Power Door Locks

### Condition:

Power door lock actuators sometimes chatter after the drivers lock cylinder is used to lock or unlock the power door locks.

### Cause:

Key code allows key to be removed in the 10 o'clock or 2 o'clock position (Figure1), causing the power door lock actuators to chatter.

### Corrective Action:

Refer to the chart on the following page to determine what the correct procedure is for correcting the condition.

#### Figure 2

R48 | R277 | R686 | T132
R78 | R447 | R719 | T137
R82 | R469 | R821 | T223
R127 | R489 | R952 | T263
R130 | R500 | -- | T347
R172 | R506 | T73 | T371
R194 | R565 | T74 | --
R196 | R675 | T121 | --
KEY CODES

#### Figure 3

R001 | R546 | T169
R246 | R584 | T179
R290 | R662 | T242
R307 | R707 | T245
R330 | R742 | T292
R412 | T030 | T323
R534 | T053 | --
REPLACEMENT KEY CODES

* For circuit inspection, refer to the Power Locks Electrical System in the Body Service Manual 1991 Edition or Power Distribution Service Manual 1991-1992 Edition

### PROCEDURE:

To record or repair lock cylinders, refer to Keys and Locks in the General Information section of the Body/Collision Repair Service Manual. Refer to Figure 3 on the previous page for the correct replacement key codes.

### Parts Requirements:

Lock Service Kit Complete 21035200

CLAIM INFORMATION | To receive credit for this repair, submit a claim through the Saturn Dealer System as follows:
--- | ---
-- | Case Type | Description | Labor Operation | Time
-- | VW | Recode All Lock Cylinders | T9554 | 3.1 hrs
Refer to the Saturn Labor Time Guide for labor codes and times for other repairs necessary.