PAINT INFORMATION - MANUFACTURERS & GENERAL REPAIR. Saturn Saturn 1994

For 1990-2009 cars

# PAINT INFORMATION - MANUFACTURERS & GENERAL REPAIR

#### SUBJECT: 1994 Model Paint Information

#### TO: The listings of 1994 paint codes contained in this bulletin will enable

Retailers to order the necessary paint materials required for proper field repairs. The list of colors indicates the suppliers' ordering codes for exterior and interior colors.

All Saturn vehicles are built at the Spring Hill, Tennessee manufacturing facility and painted with a base coat/clearcoat paint process. Paint manufacturers such as PPG, DuPont, R - M/Glasurit, Sherwin Williams-Martin Senour-Acme and AK.ZO/Sikkens produce service paint which could perform satisfactorily for field repairs. Paint suppliers in your area can provide you with information regarding these materials.

The paint listed on page 4 of this bulletin should be available from local paint suppliers.

The Service Parts Identification (SPID) label illustrated in the Figure on page 3 is located on the spare tire cover. This label contains the paint codes needed to identify the paint materials for field repairs. This label identifies the paint code along with the WA# for that paint code. It is important to use this WA# along with the paint code to identify the correct repair materials. Care should be taken to transfer the SPID label or its information if the panel to which the label is affixed requires replacement. Replacement SPID labels are not available.

The 1994 Saturn Sedans and Coupes employ composite body panels on the vertical surfaces of the vehicle. The 1994 Saturn Wagons employ composite body panels on all vertical surfaces and on the roof and tailgate. The following information identifies each type of material, where it is used and the procedures for painting the types of plastic materials used on Saturn vehicles.

Plastic Type Symbol Application ------------ ------ ----------- GTX 910 PPE+PA Fenders and Quarters PULSE ABS-PC Doors and Rockers Thermoplastic Olefin TPO Front and Rear Fascias SMC SMC Wagon Roof and Liftgate

A. Rigid Plastic Refinishing-GTX, PULSE and SMC

1. Same procedures as used for sheet metal.

2. Flex additives are not required when using urethane paint systems.

3. Avoid lacquer finishes and aggressive solvents and pre-cleaners.

B. Flexible Plastic Refinishing-TPO

1. A Polyolefin adhesion promoter such as 3M Polyolefin Adhesion Promoter (P/N 05907) or equivalent is required over all unpainted surfaces.

2. Flexible additives, used per manufacturer's recommendations, are required in primer surfacer and clearcoat.

C. Structure Painting and Touch-Up

1. Structural components are painted black with 50 percent gloss. PPG DP90 or equivalent is recommended.

2. Door openings and upper door frames are finished with a black 50 percent gloss top coat finish.

#### 1994 MODEL EXTERIOR PAINT INFORMATION

Sherwin- Williams Paint ACME-Martin- AKZO- Code Color Name WA# R-M Glasurit PPG DuPont Senour Sikkens ----------------------------------------------------------------------------- 15 Grey 9561 21064 GM-9561 4331 B9150 44119 SAT 91:15 20 Blue 9557 21060 GM-9557 4332 B9151 44121 SAT 91:20 25 Bright Aquamarine 9998 22268 GM-9998 4532 B9259 45993 SAT 92:25 28 Blue Black 9559 21062 GM-9559 4334 B9153 44123 SAT 91:28 33 Gold 5333 23000 GM-5333 4723 B9349 47134 SAT 93:33 36 Medium Blue Green 222A 24025 GM-222A 4858 B9476 48928 SAT 94:36 38 Plum 5334 23001 GM-5334 4724 B9350 47135 SAT 93:38 40 White 9563 21055 GM-9563 4336 B9155 44126 SAT 91:40 75 Medium Red 9554 21058 GM-9554 4340 B9158 44134 SAT 91:75 81 Red 9652 21057 GM-9652 4341 B9159 44135 SAT 91:81

#### 1994 MODEL INTERIOR PAINT INFORMATION

Sherwin- Paint Martin- Code Color Name WA# R-M Glasurit PPG DuPont Senour ----------------------------------------------------------------------------- 19DN Graphite 7701 13199 S/G GM-7701 DIU-33870 C8345 16963 FLT 16042 FLT UCV-2-1020 16905 S/G 16DN Neutral Grey 5302 22236 GM-5302 DIU-35395 C9267 46488 S/G UCV-2-1484 20DN Very Dk. Sapphire 8841 17094 S/G GM-8841 DIU-16202 C8770 36571 FLT 17095 FLT UCV-2-1215 36479 S/G 61 Lt. Biscuit 5347 23035 GM-5347 DIU-27524 C9343 47139 FLT UCV-2-1523 47140 S/G

Williams ACME -------- 33767 FLT 32989 S/G 46488 S/G

36571 FLT 36479 S/G 47139 FLT 47140 S/G

FLT Flat (No Gloss) S/G Semi-Gloss

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.